# Generated: 02.01.2019 19:25:17
# this file contains data for [frmFuncDevices], all lines with a # at start will be ignored
# no Errors
##############################################################################
[Controls]
btn_view_ShowAllSupportedDevices	Zeige\ alle\ unterstützten\ Geräte
l_visionsetup2	Vision\ Setup
chk_view_SmoothAutoRange	weicher\ Autorange\ \|\ Steps:
chk_view_AutorageGrenze	Autorange\ Grenze
btn_SP_ClearLog	Clear\ Log
btn_SP_OpenPort	Open\ Port
TP_SP_Text	Text
labelrecivet	Empfange\ als\ Text:
txt_SP_SendT	Test\ Text
CHK_RS232_Sonderzeichen	Sonderzeichen\ umwandeln
label_sendt	Sende:
TP_SP_Bytes	Bytes
labelreciveB	Empfange\ als\ Bytes:
txt_SP_SendB	0\ 127\ 128\ 129\ 255
labelsendb	Sende:
TP_SP_Pins	Pins
labelSP_Tab3Info	Wenn\ dieses\ Tab\ Aktiv\ ist,\ werden\ die\ Daten\ an\ andere\ Funktionen\ weitergeleitet\ und\ landen\ nicht\ im\ Terminal\.
labelSP2	2x\ Output:
label_DSR	DSR
label_CD	CD
label_CTS	CTS
btn_rs232_RTS	RTS
btn_rs232_DTR	DTR
labelsp1	3x\ Input:
l_SerialPort2	Serial\ Terminal
label2	RefTemp:\r\n\r\nRefVal:\r\n\r\nDigit/°C:
label_ArgusInfos	infos\.\.\.
l_Argus2	Device:\ Argus
btn_CEM_showCalWindow	Kalibrierfenster\ anzeigen
label_CEM_humidity	Luftfeuchte\ \(%\)
label_CEM_AtmTemp	Lufttemperatur\ \(°C\)
label_CEM_Distance	Entfernung\ \(Meter\)
label_CEM_ReflTemp	Refl\.\ Apparent\ Temp\ \(°C\)
label_CEM_info	CEM\ DT-9885\ only
label_CEM_Emiss	Emissivity
label_CEMInfos	infos\.\.\.
l_CEM2	Device:\ CEM

[conmenu]

[combo]

[UserControls]
[UC] uC_Dev_WebcamA ###########################
label_Web_HideDriverFunc	Erst\ Kamera\ starten,\ dann\ sind\ die\ Treiberfunktionen\ verfügbar\.\.\.
btn_Webcam_PropertyWin	Treiberfenster\ anzeigen
label_web_resolutions	Auflösungen:
chk_Webcam_Autoselect	Autoselect:
btn_Webcam_Start	Start
chk_WebCam_FPS	Bilder/Sec\ \(FPS\):
chk_WebCam_Resolution	Auflösung:
btn_WebCam_RefreshSources	Aktualisieren
label_web_quellen	Videoquellen:
l_Webcam2	Device:\ Webcam\ A	
[UC] uC_Dev_WebcamB ###########################
label_Web_HideDriverFunc	Erst\ Kamera\ starten,\ dann\ sind\ die\ Treiberfunktionen\ verfügbar\.\.\.
btn_Webcam_PropertyWin	Treiberfenster\ anzeigen
label_web_resolutions	Auflösungen:
chk_Webcam_Autoselect	Autoselect:
label_WebCam_Active	Webcam\ Off
btn_Webcam_Start	Start
chk_WebCam_FPS	Bilder/Sec\ \(FPS\):
chk_WebCam_Resolution	Auflösung:
btn_WebCam_RefreshSources	Aktualisieren
label_web_quellen	Videoquellen:
l_Webcam2	Device:\ Webcam\ B
[UC] uC_Dev_Flir1 ###########################
TP_FLIR_Frame	Frame
btn_flir_InitgrabIR	Init\ Grab
btn_flir_grabIR	Grab\ IR
btn_FLIR_ConnTelnet	Telnet
labeldev8	Kamera\ braucht\ RNDIS\ Modus\.
TP_FLIR_jpg	JPG
btn_flir_RecalcTemperatures	neu\ Berrechnen
chk_flirIR_DirectRead	direct
chk_flirIR_HalfSize	Half\ Size
chk_flirIR_useFileSettings	Einstellungen\ aus\ Datei\ nehmen
label_flir_ExifDatenVomBild	Exif\ Daten\ vom\ Bild
btn_Flir_CameraComanderShow	CameraCommander\ Flir\ anzeigen
chk_Flir_Autorange	Autorange
l_Flir	Device:\ Flir
cb_directReadVisual	JPG#PNG#DAT#
[UC] uC_Dev_SeekThermal1 ###########################
chk_seek_StartUpWithOpZero	Startup\ with\ Operation=0
TP_Seek1_int	Intern
btn_show_DeathPixelMap	Show\ death\ pixel\ map
label_seek_NoShutterInNormalMode	Keine\ Shutterfunktionen\r\n\ im\ Normal\ Mode
btn_seek_BigNUC	Big\ NUC
label_Seek_Proc_intern	Das\ interne\ Processing\ ist\ aktiv,\ wenn\ das\ Externe\ nicht\ eingeschaltet\ ist\.
btn_seek_NUC	NUC
btn_seek_ShutterOpen	Shutter\ Open
btn_seek_ShutterClose	Shutter\ Close
chk_seek_shutterinfo	Info\ wenn\ Shutter\ abgleich
label_rawRange	Raw\ range:
TP_Seek1_img	Img
btn_seekImg_Open	Open
label1	Reveal:\ \*\.tiff\r\nShot:\ \*\.hir\ /\ \*\.pre
label_devSeek_DevTempFrameCnt	Device\ Temp:\r\nFrame\ Count:
txt_seek_Values	MaxVal:\r\nMinVal:\r\nRange:
label_Seek_RawData	Rohdaten
chk_seek_showRawValues	Raw\ Werte\ in\ Messtabelle
label_devSeek_FWandSerial	Device\ FW:\r\nSerial:
btn_seek_initRaw	Raw
btn_seek_initHiFPS	FastRaw
label_seek_prozessierung	Prozessierung
btn_seek_initNormal	Normal
chk_seek_InitHiFPS	Init\ Hi\ FPS
btn_GetProcByteStreaming	Stream
btn_SeekThermal_Connect	Verbinden
l_Dev_SeekThermal	Device:\ SeekThermal
[UC] uC_Dev_DIYThermocam1 ###########################
chk_DIYLep_SettingsFromCamera	übernehme\ Kameraeinstellungen
btn_DIYLepton_SingleShot	Einzelbild\ aufnehmen
btn_DIYLepton_CalFileToCam	CalFile\ ->\ Kamera
btn_DIYLepton_CalCamToFile	Kamera\ ->\ CalFile
btn_DIYLepton_doNew2PCal	Neue\ 2\ Punkt\ Kalibrierung
btn_DIYLepton_WriteCalToCam	Schreibe\ Caldata\ in\ Kamera
btn_DIY_LoadCalFile	Lade
chk_DIY_UseCalFile	Benutze\ Kalibrierdatei:
btn_DIYLepton_DoNuc	NUC
btn_DIYLepton_ManNuc	Manual
btn_DIYLepton_AutoNuc	Auto
label_DIY_Shuttercontrol	Shutter\ Steuerung
btn_DIYLepton_Laser	LASER\ On/Off
label_DIYLep_SpotSensor	Spot\ Sensor
chk_DIYLep_Autoscale	Autoscale
labeldiy1	Streaming:
chk_DIYLepton_Autoselect	Auswählen,\ wenn\ da:
btn_DIYLepton_GetSize	lese\ Auflösung
btn_DIYLepton	Verbinden
label_DIY_Cal	Kalibrierung
l_Dev_DiyThermocam	Device:\ DIY\ Thermocam
CB_DIYLepton_Streaming	OFF#ThermalFrame#SpotSensor#Frame\+Spot#Visual#Visual\+Thermal#SingleShot#
CB_DIYLepton_Size	80x60#160x120#
[UC] uC_Dev_TExpert1 ###########################
label_CameraType	CameraType:
btn_TE_NUC	NUC
TP_Texp_Intern	i3\ Dll
rad_TEIR_i3Raw	Get\ Raw\ Frame
rad_TEIR_i3Temp	Get\ Temperature\ Frame
label_te_DevHandle	DeviceHandle:
btn_TEStreamingDLL	Stream
label_TE_InternProcInfo	Verbinden\ dauert\ rund\ 7\ Sek\.
btn_TExpert_ConnectDll	Verbinden
chk_UseEmisivitySetting	Emisivity:\ \r\nReflected\ Temp:
TP_Texp_WinUSB	WinUSB
chk_TE_RawToMeas	Raw->\ Meas
btn_Texp_ShowThermalExtra	Extra\ Bytes
txt_TE_Values	MaxVal:\r\nMinVal:\r\nRange:
btn_TExpert_Connect	Verbinden
btn_TEStreaming	Stream
TP_Texp_Image	Img
label_Texp_Img_desc	Einstellungen\ für\ das\ auslesen\ der\ \*\.CSV\ Bilder\ aus\ der\ Android\ APP\.
chk_TExpert_OnlyTempFrame	Nur\ TemperaturMap
chk_TExpert_SwitchSide	Bildränder\ korregieren
chk_TExpert_DiscardOvertemp	Temp\ >\ 1000°C\ ignorieren
chk_TExpert_ReplacePixelSouthEast	Ersetze\ ersten\ und\ letzten\ Pixel
l_TExpert	Device:\ i3\ T-Expert
cb_te_cameraType	TE_Q1#TE_V1#TE_M1#
[UC] uC_Dev_FlirOne1 ###########################
lblConnected	0
label19	Connected\ clients:
btn_SetPort	SET
label18	PC\ IP
lblStatus	PORT\ NOT\ OPEN
label12	Tcp\ Port
txtPort	1234
label4	Sensor
label8	Frame\ Droped\ /\ ImageTyp\r\n
l_FlirOne	Device:\ Flir\ One
[UC] uC_Dev_Testo1 ###########################
labelInfo	Only\ for\ \*\.BMT\ files\.
l_Testo	Device:\ Testo
[UC] uC_Dev_SerialSensor1 ###########################
txt_baud	115200
btn_SerSens_LoadSetup	Load
btn_SerSens_SaveSetup	Save
label_SerSens_CommandFormat	<None>\ <Command>\ <CRLF>
txt_SerSens_SendBytes	48\ 49\ 50
txt_SerSens_SendTxt	T
chk_SerSens_SendTxt	Send\ Text:
btn_SerSens_Setup	Setup
label_SerSens_Name	Name:
txt_SerSens_Name	SerSens
txt_SerSens_Value	0
txt_SerSens_Autoselect	COM10
chk_SerSens_Autoselect	Select\ if\ Exist:
btn_SerSens_Connect	Connect
l_SerialSensor	Device:\ Serial\ sensor\ 1
chk_SerSens_SendBytes	Send\ Bytes:
label2	Baud:
label1	Interval:
cb_SerSens_SensorType	Direct#Owon\ B35\ Bluetooth#Optris\ CT\ Pyrometer#
cb_SerSens_EndBytes	None#CR#CRLF#
cb_SerSens_Startbytes	None#CR#CRLF#
[UC] uC_Dev_SerialSensor2 ###########################
txt_baud	115200
btn_SerSens_LoadSetup	Load
btn_SerSens_SaveSetup	Save
label_SerSens_CommandFormat	<None>\ <Command>\ <CRLF>
txt_SerSens_SendBytes	48\ 49\ 50
txt_SerSens_SendTxt	T
chk_SerSens_SendTxt	Send\ Text:
btn_SerSens_Setup	Setup
label_SerSens_Name	Name:
txt_SerSens_Name	SerSens
txt_SerSens_Value	0
txt_SerSens_Autoselect	COM10
chk_SerSens_Autoselect	Select\ if\ Exist:
btn_SerSens_Connect	Connect
l_SerialSensor	Device:\ Serial\ sensor\ 2
chk_SerSens_SendBytes	Send\ Bytes:
label2	Baud:
label1	Interval:
cb_SerSens_SensorType	Direct#Owon\ B35\ Bluetooth#Optris\ CT\ Pyrometer#
cb_SerSens_EndBytes	None#CR#CRLF#
cb_SerSens_Startbytes	None#CR#CRLF#
[UC] uC_Dev_TCamDll1 ###########################
Btn_Tdll_ShowDPM	Show\ Death\ Pixel\ Map
TP_DLL3	DLL
txt_dll_CamConnStr	deviceConnectionString
rad_dll_ModeRaw	Raw\ Mode
rad_dll_ModeTemp	Temp\ Mode
label_dll_Log	Log:
label_dll_Name	Dll\ name\ /\ CamConnStr:
txt_dll_RelPath	TC_SeekThermal\.dll
TP_DLL4	Cmd
btn_dll_Query	Query
btn_dll_send	Send
txt_dll_send	NUC
l_TCam	Device:\ TCamDll\ 1
btn_TCam_Connect	Connect
btn_TCamStreaming	Stream
[UC] uC_Dev_TCamDll2 ###########################
Btn_Tdll_ShowDPM	Show\ Death\ Pixel\ Map
TP_DLL3	DLL
txt_dll_CamConnStr	deviceConnectionString
rad_dll_ModeRaw	Raw\ Mode
rad_dll_ModeTemp	Temp\ Mode
label_dll_Log	Log:
label_dll_Name	Dll\ name\ /\ CamConnStr:
txt_dll_RelPath	TC_SeekThermal\.dll
TP_DLL4	Cmd
btn_dll_Query	Query
btn_dll_send	Send
txt_dll_send	NUC
l_TCam	Device:\ TCamDll\ 2
btn_TCam_Connect	Connect
btn_TCamStreaming	Stream
[UC] uC_Dev_VarioCam1 ###########################
chk_EmissivityFromFile	Emissivity\ from\ file
labelInfo	Only\ for\ \*\.IRB\ files\.
l_DevName	Device:\ VarioCam
[UC] uC_Dev_BoschGtc4001 ###########################
l_DevName	Device:\ Bosch\ GTC\ 400
[UC] uC_Dev_Optris1 ###########################
TP_optris_stream	Stream
label2	RefTemp:\r\n\r\nRefVal:\r\n\r\nDigit/°C:
btn_optris_stop	Stop
chk_GetProcessedImage	Capture\ processed\ image\ as\ Visual\ \(USB\ only\)
btn_optris_connect	Connect
rad_connect_IPC2	IPC2\ \(need\ connection\ to\ Optris\ PIX\ Connect\)
rad_connect_USB	USB\ frame\ index:
TP_optris_img	Img
rad_optris_Exptif	16bit\ \.tif
rad_optris_ExpJpg	8bit\ \.jpg
label_dev_optrisexport	Export:
label_optrisInfos	infos\.\.\.
btn_optris_FolderCSV	Process\ Folder\ csv\ ->\ jpg
l_DevName	Device:\ Optris
[UC] uC_Dev_UniT1 ###########################
labelInfo	Only\ for\ \*\.BMP\ files\.
l_DevName	Device:\ Uni-T
cb_UniT_ImageMode	Auto#UTi260b#UTi85A#UTi80P#UTi690A#
[UC] uC_Dev_ThermApp1 ###########################
rad_autoscale	Autoscale
rad_ScaleFromMeta	Scale\ from\ meta
l_DevName	Device:\ ThermApp
[UC] uC_Dev_Nec1 ###########################
l_Nec	Device:\ Nec
[UC] uC_Dev_DjiDrohne1 ###########################
labelInfo	For\ \*\.jpg\ files\.
l_Testo	Device:\ DJI\ Drohne

